{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Quat inno tech","Quạt Windy"],"not_rendered":{"charts":0,"images":54,"macros":1,"external_links":1,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Quat inno tech","index":0,"n_rows":324,"n_cols":10,"rows_kept":324,"cut":false,"hidden":false,"merged":[[487,0,489,0],[487,5,492,5],[490,0,491,0],[493,5,495,5],[494,0,495,0],[461,0,466,0],[461,5,468,5],[467,0,470,0],[469,5,479,5],[472,0,478,0],[479,0,482,0],[481,5,486,5],[483,0,486,0],[435,5,442,5],[437,7,439,7],[446,0,458,0],[446,5,453,5],[454,5,460,5],[459,0,460,0],[405,5,408,5],[412,0,412,10],[414,0,423,0],[414,5,421,5],[422,5,429,5],[424,0,433,0],[426,7,429,7],[430,5,434,5],[434,0,442,0],[358,0,383,0],[358,5,371,5],[372,5,385,5],[384,0,401,0],[386,5,396,5],[397,5,402,5],[402,0,404,0],[403,5,404,5],[305,0,307,0],[305,1,307,1],[305,8,306,8],[305,9,306,9],[307,2,307,9],[309,0,311,0],[309,1,311,1],[309,8,310,8],[309,9,310,9],[311,2,311,9],[297,0,298,0],[297,1,301,1],[297,8,298,8],[297,9,298,9],[299,0,300,0],[302,0,304,0],[294,8,295,8],[294,9,295,9],[296,2,296,9],[302,1,304,1],[302,8,303,8],[302,9,303,9],[304,2,304,9],[299,8,300,8],[299,9,300,9],[301,2,301,9],[283,9,284,9],[285,9,286,9],[281,8,282,8],[283,8,284,8],[285,8,286,8],[292,0,293,0],[292,1,296,1],[292,8,293,8],[292,9,293,9],[294,0,295,0],[279,0,280,0],[279,8,280,8],[279,9,280,9],[278,2,278,9],[287,0,288,0],[289,0,290,0],[287,9,288,9],[289,8,290,8],[289,9,290,9],[281,9,282,9],[276,8,277,8],[291,2,291,9],[281,0,282,0],[283,0,284,0],[285,0,286,0],[279,1,286,1],[276,9,277,9],[276,1,278,1],[287,1,291,1],[287,8,288,8],[231,0,232,0],[233,0,234,0],[235,0,236,0],[237,0,238,0],[231,9,232,9],[231,1,238,1],[231,8,232,8],[237,8,238,8],[235,9,236,9],[233,9,234,9],[239,9,242,9],[243,9,246,9],[239,8,242,8],[237,9,238,9],[189,9,190,9],[183,9,184,9],[185,9,186,9],[197,8,198,8],[197,9,198,9],[207,8,208,8],[187,9,188,9],[201,8,202,8],[312,1,317,1],[312,8,313,8],[312,9,313,9],[314,8,315,8],[314,9,315,9],[316,8,317,8],[316,9,317,9],[165,1,169,1],[165,0,166,0],[167,0,168,0],[165,8,166,8],[169,2,169,9],[160,1,164,1],[160,0,161,0],[162,0,163,0],[160,8,161,8],[162,8,163,8],[174,9,175,9],[160,9,161,9],[162,9,163,9],[233,8,234,8],[165,9,166,9],[167,8,168,8],[167,9,168,9],[182,2,182,9],[201,9,202,9],[199,8,200,8],[158,0,159,0],[148,9,149,9],[148,8,149,8],[146,1,150,1],[146,0,147,0],[148,0,149,0],[146,8,147,8],[152,1,159,1],[152,8,153,8],[152,9,153,9],[152,0,153,0],[154,0,155,0],[156,0,157,0],[154,8,155,8],[154,9,155,9],[156,8,157,8],[156,9,157,9],[141,1,145,1],[141,0,142,0],[143,0,144,0],[141,8,142,8],[143,8,144,8],[145,2,145,9],[141,9,142,9],[143,9,144,9],[5,0,6,0],[5,1,9,1],[5,8,6,8],[5,9,6,9],[7,0,8,0],[7,8,8,8],[0,0,0,9],[2,0,2,1],[2,2,2,8],[7,9,8,9],[10,0,11,0],[10,1,14,1],[10,8,11,8],[10,9,11,9],[12,0,13,0],[12,8,13,8],[12,9,13,9],[15,0,16,0],[15,1,20,1],[15,8,16,8],[15,9,16,9],[17,0,18,0],[17,8,18,8],[17,9,18,9],[19,0,20,0],[19,8,20,8],[19,9,20,9],[21,0,22,0],[21,1,26,1],[21,8,22,8],[21,9,22,9],[23,0,24,0],[23,8,24,8],[23,9,24,9],[25,0,26,0],[25,8,26,8],[25,9,26,9],[27,0,28,0],[27,1,34,1],[27,8,28,8],[27,9,28,9],[29,0,30,0],[29,8,30,8],[29,9,30,9],[31,0,32,0],[31,8,32,8],[31,9,32,9],[33,0,34,0],[33,8,34,8],[33,9,34,9],[35,0,36,0],[35,1,42,1],[35,8,36,8],[35,9,36,9],[37,0,38,0],[37,8,38,8],[37,9,38,9],[39,0,40,0],[39,8,40,8],[39,9,40,9],[41,0,42,0],[41,8,42,8],[41,9,42,9],[44,0,45,0],[44,1,48,1],[46,0,47,0],[48,2,48,9],[49,9,50,9],[51,9,52,9],[53,2,53,9],[44,8,45,8],[46,8,47,8],[44,9,45,9],[46,9,47,9],[49,0,50,0],[49,1,53,1],[51,0,52,0],[49,8,50,8],[51,8,52,8],[54,1,58,1],[54,0,55,0],[56,0,57,0],[54,8,55,8],[58,2,58,9],[54,9,55,9],[56,8,57,8],[56,9,57,9],[59,9,60,9],[61,8,62,8],[61,9,62,9],[261,2,261,9],[264,2,264,9],[72,9,73,9],[74,8,75,8],[74,9,75,9],[70,8,71,8],[146,9,147,9],[275,2,275,9],[66,0,67,0],[68,0,69,0],[64,1,69,1],[63,2,63,9],[64,8,65,8],[59,1,63,1],[59,0,60,0],[61,0,62,0],[59,8,60,8],[64,0,65,0],[64,9,65,9],[66,8,67,8],[66,9,67,9],[68,8,69,8],[68,9,69,9],[70,9,71,9],[83,8,84,8],[74,0,75,0],[70,1,75,1],[72,8,73,8],[72,0,73,0],[70,0,71,0],[77,9,78,9],[79,9,80,9],[81,9,82,9],[85,9,86,9],[87,9,88,9],[77,0,78,0],[79,0,80,0],[81,0,82,0],[83,0,84,0],[77,1,84,1],[77,8,78,8],[79,8,80,8],[81,8,82,8],[83,9,84,9],[89,9,90,9],[91,9,92,9],[85,0,86,0],[85,1,94,1],[87,8,88,8],[89,8,90,8],[91,8,92,8],[93,8,94,8],[85,8,86,8],[89,0,90,0],[91,0,92,0],[106,0,107,0],[87,0,88,0],[93,9,94,9],[96,0,97,0],[96,1,100,1],[96,8,97,8],[96,9,97,9],[93,0,94,0],[110,0,111,0],[112,0,113,0],[118,8,119,8],[114,0,115,0],[116,0,117,0],[118,0,119,0],[118,9,119,9],[120,0,121,0],[122,0,123,0],[106,1,123,1],[106,8,107,8],[106,9,107,9],[108,8,109,8],[108,9,109,9],[110,9,111,9],[112,9,113,9],[116,9,117,9],[101,1,105,1],[98,0,99,0],[98,8,99,8],[98,9,99,9],[101,0,102,0],[103,0,104,0],[110,8,111,8],[112,8,113,8],[108,0,109,0],[101,8,102,8],[103,8,104,8],[103,9,104,9],[101,9,102,9],[124,0,125,0],[126,0,127,0],[126,9,127,9],[114,9,115,9],[114,8,115,8],[116,8,117,8],[128,0,129,0],[120,9,121,9],[120,8,121,8],[122,8,123,8],[122,9,123,9],[130,0,131,0],[124,1,131,1],[124,8,125,8],[124,9,125,9],[126,8,127,8],[128,8,129,8],[128,9,129,9],[130,8,131,8],[130,9,131,9],[133,1,140,1],[133,0,134,0],[135,0,136,0],[137,0,138,0],[139,0,140,0],[133,9,134,9],[135,8,136,8],[135,9,136,9],[170,9,171,9],[137,8,138,8],[137,9,138,9],[139,8,140,8],[139,9,140,9],[164,2,164,9],[158,8,159,8],[158,9,159,9],[133,8,134,8],[150,2,150,9],[176,8,177,8],[176,9,177,9],[170,1,177,1],[170,0,171,0],[174,0,175,0],[170,8,171,8],[172,8,173,8],[172,9,173,9],[176,0,177,0],[172,0,173,0],[178,0,179,0],[180,0,181,0],[178,8,179,8],[178,9,179,9],[180,8,181,8],[180,9,181,9],[178,1,182,1],[174,8,175,8],[183,0,184,0],[185,0,186,0],[187,0,188,0],[189,0,190,0],[183,1,190,1],[183,8,184,8],[185,8,186,8],[187,8,188,8],[189,8,190,8],[211,0,212,0],[213,8,214,8],[197,0,198,0],[199,0,200,0],[201,0,202,0],[258,2,258,9],[239,1,246,1],[217,2,217,9],[243,8,246,8],[235,8,236,8],[195,2,195,9],[318,0,319,0],[312,0,313,0],[314,0,315,0],[316,0,317,0],[239,0,242,0],[243,0,246,0],[276,0,278,0],[247,0,250,0],[251,0,254,0],[256,0,258,0],[199,9,200,9],[318,9,319,9],[320,0,321,0],[320,8,321,8],[320,9,321,9],[318,1,323,1],[318,8,319,8],[203,0,204,0],[209,0,210,0],[209,9,210,9],[211,8,212,8],[211,9,212,9],[205,1,212,1],[203,8,204,8],[203,9,204,9],[205,8,206,8],[205,9,206,9],[207,9,208,9],[209,8,210,8],[215,9,216,9],[229,0,230,0],[218,1,222,1],[218,0,219,0],[220,0,221,0],[218,8,219,8],[218,9,219,9],[220,8,221,8],[222,2,222,9],[227,0,228,0],[191,0,192,0],[191,1,195,1],[193,0,194,0],[223,1,230,1],[213,1,217,1],[213,0,214,0],[215,0,216,0],[205,0,206,0],[207,0,208,0],[197,1,204,1],[220,9,221,9],[225,9,226,9],[223,0,224,0],[225,0,226,0],[191,8,192,8],[191,9,192,9],[193,8,194,8],[193,9,194,9],[213,9,214,9],[215,8,216,8],[227,9,228,9],[229,8,230,8],[229,9,230,9],[223,8,224,8],[223,9,224,9],[225,8,226,8],[227,8,228,8],[247,8,250,8],[247,9,250,9],[251,8,254,8],[251,9,254,9],[247,1,254,1],[259,8,260,8],[259,9,260,9],[256,8,257,8],[256,9,257,9],[256,1,258,1],[259,1,261,1],[259,0,261,0],[262,1,264,1],[262,0,264,0],[262,8,263,8],[262,9,263,9],[273,8,274,8],[273,9,274,9],[271,8,272,8],[265,0,267,0],[265,1,267,1],[265,8,266,8],[265,9,266,9],[271,9,272,9],[267,2,267,9],[322,0,323,0],[322,8,323,8],[322,9,323,9],[268,0,270,0],[268,1,270,1],[268,8,269,8],[268,9,269,9],[271,1,275,1],[271,0,272,0],[273,0,274,0]],"flags":["formulas_cached_only"]}
["BẢNG THÔNG TIN QUẠT INNO TECH"]
[]
["Sản Phẩm",null,"Thông số kỹ thuật"]
["Model","Hình ảnh","Power\n(∮/V/Hz)","I \n(A)","P \n(W)","Q \n(m3/h)","Áp lực\n(mmAq)","T. độ\n(Rpm)","T. ồn\n(dB)","m\n(Kg)"]
["Quạt thổi khí áp suất cao đa cấp (Hight-pressure multilevel blowers)"]
["ITB-S411S",null,"1/220/60",7.5,1750,1620,300,3400,80,24]
[null,null,"1/220/50",5.3,1100,1380,226,2900]
["ITB-S411T",null,"3/220-380/60","5.3/2.9",1750,1620,300,3370,80,24]
[null,null,"3/220-380/50","4.1/2.3",1100,1380,226,2900]
[]
["ITB-411S",null,"1/220/60",7.5,1750,1620,300,3400,80,23]
[null,null,"1/220/50",5.3,1100,1380,226,2900]
["ITB-411T",null,"3/220-380/60","5.3/2.9",1750,1620,300,3370,80,23]
[null,null,"3/220-380/50","4.1/2.3",1100,1380,226,2900]
[]
["ITB-412T",null,"3/220-380/60","6.4/3.6",2050,1200,555,3400,82,32]
[null,null,"3/220-380/50","5.6/3.3",1330,1020,405,2900]
["ITB-413T",null,"3/220-380/60","8.2/5.0",2650,1200,725,3459,85,38]
[null,null,"3/220-380/50","8.2/4.5",1780,1020,510,2940]
["ITB-414T",null,"3/220-380/60","11/6.08",3300,1200,1100,3485,86,42]
[null,null,"3/220-380/50","9.0/5.0",2200,1020,775,2920]
["ITB-S412T",null,"3/220-380/60","6.4/3.6",2050,1200,555,3400,82,33]
[null,null,"3/220-380/50","5.6/3.3",1330,1020,405,2900]
["ITB-S413T",null,"3/220-380/60","8.2/5.0",2650,1200,725,3459,85,39]
[null,null,"3/220-380/50","8.2/4.5",1780,1020,510,2094]
["ITB-S414T",null,"3/220-380/60","11/6.08",3300,1200,1100,3485,86,43]
[null,null,"3/220-380/50","9.0/5.0",2200,1020,775,2920]
["ITB-401S",null,"1/220/60",4.95,1080,600,352,3435,83,20.5]
[null,null,"1/220/50",3.6,725,510,260,2925]
["ITB-401T",null,"3/220-380/60","3.3/1.9",1180,600,352,3390,83,20.5]
[null,null,"3/220-380/50","2.1/1.4",735,510,260,2920]
["ITB-402S",null,"1/220/60",6.9,1525,630,635,3480,83,25.5]
[null,null,"1/220/50",5.85,1330,540,465,2938]
["ITB-402T",null,"3/220-380/60","4.7/2.65",1610,630,635,3450,83,25.5]
[null,null,"3/220-380/50","3.25/1.9",900,540,465,2942]
["ITB-S401S",null,"1/220/60",4.95,1080,600,352,3435,83,21.5]
[null,null,"1/220/50",3.6,725,510,260,2925]
["ITB-S401T",null,"3/220-380/60","3.3/1.9",1180,600,352,3390,83,21.5]
[null,null,"3/220-380/50","2.1/1.4",735,510,260,2920]
["ITB-S402S",null,"1/220/60",6.9,1525,630,635,3480,83,26.5]
[null,null,"1/220/50",5.85,1330,540,465,2938]
["ITB-S402T",null,"3/220-380/60","4.7/2.65",1610,630,635,3450,83,26.5]
[null,null,"3/220-380/50","3.25/1.9",900,540,465,2942]
["Sò cao áp (Turbo blowers)"]
["TBS-3235S",null,"1/220/60",4.7,1300,1560,265,3410,83,35]
[null,null,"1/220/50",3.8,900,1365,196,2850]
["TBS-3235T",null,"3/220-380/60","3.1/1.8",1300,1560,265,3410,83,35]
[null,null,"3/220-380/50","2.6/1.5",856,1365,196,2850,2850]
[null,null,"1HP"]
["TBS-S3235S",null,"1/220/60",4.7,1300,1560,265,3410,83,35.5]
[null,null,"1/220/50",3.8,900,1365,196,2850,2850]
["TBS-S3235T",null,"3/220-380/60","3.1/1.8",1300,1560,265,3410,83,35.5]
[null,null,"3/220-380/50","2.6/1.5",856,1365,196,2850,2850]
[null,null,"1HP"]
["TBS-3245S",null,"1/220/60",7,1800,2400,285,3460,87,40]
[null,null,"1/220/50",5.7,1540,2100,210,2920,2850]
["TBS-3245T",null,"3/220-380/60","4.5/2.6",1800,2400,285,3460,87,40]
[null,null,"3/220-380/50","3.7/2.2",1540,2100,210,2920,2850]
[null,null,"2HP"]
["TBS-S3245S",null,"1/220/60",7,1800,2400,285,3460,87,40]
[null,null,"1/220/50",5.7,1540,2100,210,2920,2850]
["TBS-S3245S",null,"3/220-380/60","4.5/2.6",1800,2400,285,3460,87,40]
[null,null,"3/220-380/50","3.7/2.2",1540,2100,210,2920,2850]
[null,null,"2HP"]
["TBS-3735S\n(3HP)",null,"1/220/60",8.2,2800,3120,320,3450,90,45]
[null,null,"1/220/50",7,2300,2730,237,2915]
["TBS-3735T\n(3HP)",null,"3/220-380/60","5.3/3.1",2800,3120,320,3450,90,45]
[null,null,"3/220-380/50","4.5/2.6",2300,2730,237,2915]
["TBS-3765T\n(5HP)",null,"3/220-380/60","13/7.7",4200,4020,380,3460,92,50]
[null,null,"3/220-380/50","11/6.3",3400,3510,280,2980]
["TBS-S3735S\n(3HP)",null,"1/220/60",8.2,2800,3120,320,3450,90,46]
[null,null,"1/220/50",7,2300,2730,237,2915]
["TBS-S3735T\n(3HP)",null,"3/220-380/60","5.3/3.1",2800,3120,320,3450,90,46]
[null,null,"3/220-380/50","4.5/2.6",2300,2730,237,2915]
["TBS-S3765T\n(5HP)",null,"3/220-380/60","13/7.7",4200,4020,380,3460,92,51]
[null,null,"3/220-380/50","11/6.3",3400,3510,280,2980]
["Cabinet fans-Double inlet & blower for dust collectors"]
["ITC-230GS",null,"1/220/60",1.3,320,1800,24,1160,61,26]
[null,null,"1/220/50",1.2,190,1440,16,960]
["ITC-230GT",null,"3/220-380/60","1.0/0.6",240,1800,24,1150,61,26]
[null,null,"3/220-380/50","0.6/0.36",170,1440,16,950]
["ITC-250GS",null,"1/220/60",2.8,570,2900,35,1100,63,33]
[null,null,"1/220/50",1.68,340,2320,24,940]
["ITC-250GT",null,"3/220-380/60","2.6/1.6",560,2900,35,1120,63,33]
[null,null,"3/220-380/50","1.56/0.96",390,2320,24,945]
["ITC-300GS",null,"1/220/60",5.9,1190,4500,50,1120,68,51]
[null,null,"1/220/50",4,710,3800,37,960]
["ITC-300GT",null,"3/220-380/60","5.7.0/3.4",1140,4500,50,1145,68,51]
[null,null,"3/220-380/50","3.8/2.3",680,3800,37,970]
["ITC-380HS",null,"1/220/60",7.5,1500,8500,54,810,70,66]
[null,null,"1/220/50",5.2,910,7100,46,710]
["ITC-380HT",null,"3/220-380/60","7.3/3.1",1450,8500,54,815,70,66]
[null,null,"3/220-380/50","5.1/2.2",870,7100,46,720]
["ITC-400GT",null,"3/220-380/60","16.5/9.9",3500,12000,88,1100,75,66]
[null,null,"3/220-380/50","11.5/6.8",2100,10200,73,950]
[" Sò nhỏ (Small sirocco blowers)"]
["TIS-140FS",null,"1/220/60",0.3,60,510,12,1365,42,4.5]
[null,null,"1/220/50",0.2,48,443,9.3,1335,53]
["TIS-160FS",null,"1/220/60",0.6,131,900,20,1350,53,7]
[null,null,"1/220/50",0.5,105,783,15.5,1335]
[]
["TIS-190FS",null,"1/220/60",1.6,360,1260,31,1530,56,10.5]
[null,null,"1/220/50",1.3,288,1090,24,1410]
["TIS-190FT",null,"3/220-380/60","2.1/1.2",360,1260,31,1510,56,10.5]
[null,null,"3/220-380/50","0.9/0.7",278,1090,24,1395]
[]
["TIS-250GS\n(Ø250 x 130)",null,"1/220/60",2.1,428,2520,25,1130,60,20.3]
[null,null,"1/220/50",1.9,342,2190,19,985]
["TIS-250GT\n(Ø250 x 130)",null,"3/220-380/60","2.1/1.4",428,2520,25,1150,60,20.3]
[null,null,"3/220-380/50","2.3/1.4",328,2190,19,990]
["TIS-280FS\n(Ø250 x 130)",null,"1/220/60",5.8,1280,3600,45,1725,64,22.3]
[null,null,"1/220/50",5.2,935,3060,35,1460]
["TIS-280FT\n(Ø250 x 130)",null,"3/220-380/60","4.1/2.4",1280,3600,45,1710,64,22.3]
[null,null,"3/220-380/50","2.9/1.7",890,3060,35,1455]
["TIS-280GS\n(Ø250 x 150)",null,"1/220/60",2.3,514,3240,27,1125,62,22.3]
[null,null,"1/220/50",2.1,412,2820,21,980]
["TIS-280GT\n(Ø250 x 150)",null,"3/220-380/60","2.2/1.3",514,3240,27,1150,62,22.3]
[null,null,"3/220-380/50","2.4/1.3",398,2820,21,985]
["TIS-290FS\n(Ø250 x 150)",null,"1/220/60",6.8,1420,4680,53,1690,72,25]
[null,null,"1/220/50",5.9,1190,3970,41,1450]
["TIS-290FT\n(Ø250 x 150)",null,"3/220-380/60","4.7/2.8",1420,4680,53,1710,72,25]
[null,null,"3/220-380/50","4.9/2.7",1205,3970,41,1460]
["TIS-290GS\n(Ø250 x 150)",null,"1/220/60",2.4,530,3300,23,1145,63,25]
[null,null,"1/220/50",2.2,424,2870,18,985]
["TIS-S250GS",null,"1/220/60",2.1,428,2520,25,1130,60,20.3]
[null,null,"1/220/50",1.9,342,2190,19,985]
["TIS-S250GT",null,"3/220-380/60","2.1/1.4",428,2520,25,1150,60,20.3]
[null,null,"3/220-380/50","2.3/1.4",328,2190,19,990]
["TIS-S280FS",null,"1/220/60",5.8,1280,3600,45,1725,64,22.3]
[null,null,"1/220/50",5.2,935,3060,35,1460]
["TIS-S280FT",null,"3/220-380/60","4.1/2.4",1280,3600,45,1710,64,22.3]
[null,null,"3/220-380/50","2.9/1.7",890,3060,35,1455]
[" Sò lồng sóc lớn (Large sirocco blowers)"]
["TIS-310GS",null,"1/220/60",5.9,1200,5670,21,1130,65,51]
[null,null,"1/220/50",4.9,890,4875,16,950]
["TIS-310GT",null,"3/220-380/60","4.1/2.4",1200,5670,21,1135,65,51]
[null,null,"3/220-380/50","3.3/1.8",830,4875,16,955]
["TIS-370GS",null,"1/220/60",11.4,2400,8580,40,1115,67,54]
[null,null,"1/220/50",8.7,1790,7200,30,965]
["TIS-370GT",null,"3/220-380/60","9.2/5.8",2400,8580,40,1110,67,54]
[null,null,"3/220-380/50","7.1/3.7",1690,7200,30,960]
["TIS-B310FS",null,"1/220/60",8.2,1800,7000,35,1690,66,52]
[null,null,"1/220/50",7.6,1335,5985,27,1450]
["TIS-B310FT",null,"3/220-380/440/60","6.1/3.6",1830,7000,35,1710,66,52]
[null,null,"3/220-380/440/50","4.3/2.6",1305,5985,27,1460]
[null,null,"Kích thước cánh quạt (mm): Ø310 x 165"]
["TIS-390GT",null,"3/220-380/60","9.5/7.5",3500,11800,42,1150,69,68]
[null,null,"3/220-380/50","8.7/4.9",2270,9900,31,980]
["TIS-390HT",null,"3/220-380/60","5.1/2.9",1700,7800,22,880,65,68]
[null,null,"3/220-380/50","4.3/2.6",1428,6550,17,755]
[null,null,"Kích thước cánh quạt (mm): Ø390 x 170"]
["Quạt hướng trục thân tròn (Portable fans)"]
["TIP-200S\n(Ø170 mm)",null,"1/220/60",0.8,190,1140,30,3280,61,6.5]
[null,null,"1/220/50",0.7,140,1250,23,2840]
["TIP-250S\n(Ø220 mm)",null,"1/220/60",1.3,310,3060,38,3410,65,7.6]
[null,null,"1/220/50",1.1,230,2660,29,2950]
["TIP-300S\n(Ø270 mm)",null,"1/220/60",1.9,440,3780,50,3300,67,11]
[null,null,"1/220/50",1.5,325,3280,38,2850]
["TIP-350S\n(Ø320 mm)",null,"1/220/60",4.1,890,6900,80,3420,70,18]
[null,null,"1/220/50",3.1,658,6010,60,2960]
["TIP-250S-1",null,"1/220/60",1.3,310,3060,38,3410,65,7.6]
[null,null,"1/220/50",1.1,230,2660,29,2950]
["TIP-300S-1",null,"1/220/60",1.9,440,3780,50,3300,67,11]
[null,null,"1/220/50",1.5,325,3280,38,2850]
[null,null,"Kích thước cánh quạt (mm): TIP-250S-1 (Ø220 mm); TIP-300S-1 (Ø270 mm)"]
["TIP-400S",null,"1/220/60",0.8,400,6060,30,1620,66,22.8]
[null,null,"1/220/50",0.7,280,5272,23,1415]
["TIP-500S",null,"1/220/60",4.8,990,10560,39,1680,69,31.2]
[null,null,"1/220/50",3.3,690,8970,29,1465]
[null,null,"Kích thước cánh quạt (mm): TIP-400S (Ø370 mm); TIP-500S (Ø470 mm)"]
["TIP-400S-1\n(Ø370 mm)",null,"1/220/60",1.9,400,6060,30,1620,66,24.2]
[null,null,"1/220/50",1.4,280,5272,23,1415]
["TIP-400T-1\n(Ø370 mm)",null,"3/220-380/60","1.5/0.9",400,6060,30,1650,66,24.2]
[null,null,"3/220-380/50","1.6/1.0",280,5272,23,1435]
["TIP-500S-1\n(Ø470 mm)",null,"1/220/60",4.8,990,10560,39,1680,69,34.6]
[null,null,"1/220/50",3.3,690,8970,29,1465]
["TIP-500T-1\n(Ø470 mm)",null,"3/220-380/60","6.2/3.3",990,10560,39,1690,69,34.6]
[null,null,"3/220-380/50","3.6/2.2",690,8970,29,1455]
["TIP-600S-1",null,"1/220/60",6.4,1400,25200,60,1620,88,57]
[null,null,"1/220/50",3.8,850,21000,43,1415]
["TIP-600T-1",null,"3/220-380/60","6.2/3.3",1260,25200,60,1650,88,57]
[null,null,"3/220-380/50","3.6/2.2",850,21300,43,1415]
[null,null,"Kích thước cánh quạt (mm): Ø600 mm"]
["TIP-400D\n(Ø370 mm)",null,"1/220/60",1.9,400,6060,30,1620,66,14.5]
[null,null,"1/220/50",1.4,280,5272,23,1415]
["TIP-400DT\n(Ø370 mm)",null,"3/220-380/60","1.5/0.9",400,6060,30,1650,66,15.5]
[null,null,"3/220-380/50","1.6/1.0",280,5272,23,1435]
["TIP-500D\n(Ø470 mm)",null,"1/220/60",4.8,990,10560,39,1680,69,23]
[null,null,"1/220/50",3.3,690,8970,29,1465]
["TIP-500DT\n(Ø470 mm)",null,"3/220-380/60","3.2/1.9",990,10560,39,1690,69,23]
[null,null,"3/220-380/50","3.2/1.8",690,8970,29,1455]
["TIP-600DS",null,"1/220/60",2,439,15600,29,1130,66,33]
[null,null,"1/220/50",1.5,315,13200,21,985]
["TIP-600DT",null,"3/220-380/60","1.4/0.8",439,15600,29,1120,66,33]
[null,null,"3/220-380/50","1.0/0.6",315,13200,21,965]
[null,null,"Kích thước cánh quạt (mm): Ø600 mm"]
["Quạt thổi áp lực cao (High-pressure blowers)"]
["TBS-230\n(Ø20.5 cm)",null,"1/220/60",1.9,330,660,120,3440,83,12]
[null,null,"1/220/50",1.4,220,570,90,2970]
["TBT-230\nØ20.5 cm)",null,"3/220-380/60","1.5/0.9",340,660,120,3300,83,12]
[null,null,"3/220-380/50","1.6/1.0",260,570,90,2850]
["TBS-270\nØ24.5 cm)",null,"1/220/60",4.8,680,1200,170,3430,80,15]
[null,null,"1/220/50",3.3,500,1080,130,2960]
["TBT-270\nØ24.5 cm)",null,"3/220-380/60","3.2/1.9",670,1200,170,3430,80,15]
[null,null,"3/220-380/50","3.2/1.8",470,1080,130,2960]
["TBS-230S\n(Ø20.5 cm)",null,"1/220/60",1.9,330,660,120,3440,83,12.5]
[null,null,"1/220/50",1.4,220,570,90,2970]
["TBT-230S\nØ20.5 cm)",null,"3/220-380/60","1.5/0.9",340,660,120,3300,83,12.5]
[null,null,"3/220-380/50","1.6/1.0",260,570,90,2850]
["TBS-270S\nØ24.5 cm)",null,"1/220/60",4.8,680,1200,170,3430,80,15.5]
[null,null,"1/220/50",3.3,500,1080,130,2960]
["TBT-270S\nØ24.5 cm)",null,"3/220-380/60","3.2/1.9",670,1200,170,3430,80,15.5]
[null,null,"3/220-380/50","3.2/1.8",470,1080,130,2960]
["TBS-300",null,"1/220/60",4.8,840,1380,190,3350,76,18.5]
[null,null,"1/220/50",3.3,570,1200,145,2890]
["TBT-300",null,"3/220-380/60","3.2/1.9",850,1380,190,3360,76,18.5]
[null,null,"3/220-380/50","3.2/1.8",570,1200,145,2890]
[null,null,"Kích thước cánh quạt (mm): Ø275 mm"]
["TBS-300S",null,"1/220/60",4.8,840,1380,190,3350,76,19]
[null,null,"1/220/50",3.3,570,1200,145,2890]
["TBT-300S",null,"3/220-380/60","3.2/1.9",850,1380,190,3360,76,19]
[null,null,"3/220-380/50","3.2/1.8",570,1200,145,2890]
[null,null,"Kích thước cánh quạt (mm): Ø275 mm"]
["TBS-301\n(Ø275 mm)",null,"1/220/60",4.4,1010,1620,206,3430,85,19]
[null,null,"1/220/50",3.3,675,1380,155,2960]
["TBT-301\n(Ø275 mm)",null,"3/220-380/60","3.0/1.8",1030,1620,206,3430,85,19]
[null,null,"3/220-380/50","1.6/1.0",650,1380,155,2960]
["TBS-302\n(Ø275 mm)",null,"1/220/60",4.8,1050,1710,215,3450,86,20]
[null,null,"1/220/50",3.3,720,1500,165,2960]
["TBT-301\n(Ø275 mm)",null,"3/220-380/60","4.0/2.3",1050,1710,215,3450,86,20]
[null,null,"3/220-380/50","3.5/2.0",570,1500,165,2960]
["TBS-301S\n(Ø275 mm)",null,"1/220/60",4.4,1010,1620,206,3430,85,19]
[null,null,"1/220/50",3.3,675,1380,155,2960]
["TBT-301S\n(Ø275 mm)",null,"3/220-380/60","3.0/1.8",1030,1620,206,3430,85,19]
[null,null,"3/220-380/50","1.6/1.0",650,1380,155,2960]
["TBS-302S\n(Ø275 mm)",null,"1/220/60",4.8,1050,1710,215,3450,86,20.5]
[null,null,"1/220/50",3.3,720,1500,165,2960]
["TBT-302S\n(Ø275 mm)",null,"3/220-380/60","4.0/2.3",1050,1710,215,3450,86,20.5]
[null,null,"3/220-380/50","3.5/2.0",570,1500,165,2960]
["TB-2B\n(Ø185 mm)",null,"1/220/60",2.35,510,1050,120,3400,68,12]
[null,null,"1/220/50",1.7,350,900,90,2920]
[null,null,"3/220-380/60","1.62/0.9",510,1050,120,3350]
[null,null,"3/220-380/50","1.2/0.7",360,900,90,2920]
["TB-4B\n(Ø150 mm)",null,"1/220/60",1,210,426,75,3400,67,7.5]
[null,null,"1/220/50",0.8,180,360,50,2900]
[null,null,"3/220-380/60","0.75/0.42",230,426,75,3400,86,20.5]
[null,null,"3/220-380/50","0.9/0.5",210,360,50,2900]
["TB-2S\n(Ø185 mm)",null,"1/220/60",2.35,510,1050,120,3400,68,12.5]
[null,null,"1/220/50",1.7,350,900,90,2920]
[null,null,"3/220-380/60","1.62/0.9",510,1050,120,3350]
[null,null,"3/220-380/50","1.2/0.7",360,900,90,2920]
["TB-4S\n(Ø150 mm)",null,"1/220/60",1,210,426,75,3400,67,8]
[null,null,"1/220/50",0.8,180,360,50,2900]
[null,null,"3/220-380/60","0.75/0.42",230,426,75,3400,86,20.5]
[null,null,"3/220-380/50","0.9/0.5",210,360,50,2900]
["Sò thổi nhỏ (Small blowers)"]
["TB-75",null,"1/220/60",0.21,29,84,16,2350,35,0.9]
[null,null,"1/220/50",0.2,23,78,14,2245]
[null,null,"Kích thước cánh quạt (mm): Ø85 x 70"]
["TB-95",null,"1/220/60",0.19,40,162,22,3140,39,1.3]
[null,null,"1/220/50",0.18,32,128,18,2730]
[null,null,"Kích thước cánh quạt (mm): Ø88 x 40"]
["TB-105",null,"1/220/60",0.31,60,300,37,3070,42,2.1]
[null,null,"1/220/50",0.26,48,240,32,2730]
[null,null,"Kích thước cánh quạt (mm): Ø105 x 50"]
["TB-105F",null,"1/220/60",0.31,60,300,37,3070,42,2.1]
[null,null,"1/220/50",0.26,48,270,32,2730]
[null,null,"Kích thước cánh quạt (mm): Ø105 x 50"]
["TB-118",null,"1/220/60",0.49,100,360,43,3380,58,3.3]
[null,null,"1/220/50",0.48,91,324,30,2910]
[null,null,"Kích thước cánh quạt (mm): Ø115 x 50"]
["TB-95-1",null,"1/220/60",0.19,40,162,22,3450,39,1.3]
[null,null,"1/220/50",0.18,32,128,18,2960]
["TB-115",null,"1/220/60",0.31,60,300,37,3450,42,2.1]
[null,null,"1/220/50",0.26,48,240,32,2960]
[null,null,"Kích thước cánh quạt (mm): TB-95-1: Ø88 x 40; TB-115: Ø105 x 50"]
[" TB-118-1",null,"1/220/60",0.49,100,360,43,3380,58,3.3]
[null,null,"1/220/50",0.48,91,324,30,2910]
[null,null,"Kích thước cánh quạt (mm): Ø115 x 50"]
["  TB-150\nØ118x60",null,"1/220/60",0.9,209,480,49,3470,62,6.4]
[null,null,"1/220/50",0.84,167,406,37,2895]
["TB-150(3∮)\nØ118x60",null,"3/220-380/60","0.85/0.75",209,480,49,3410,62,6.4]
[null,null,"1/220/50","0.8/0.6",152,406,37,2900]
["TB-200\nØ148x80",null,"3/220-380/60",2.3,485,960,79,3275,64,9]
[null,null,"1/220/50",1.8,367,844,62,2865]
["TB-200(3∮)\nØ148x80",null,"3/220-380/60","1.6/0.9",485,960,79,3320,64,9]
[null,null,"1/220/50","1.7/1.0",386,844,62,2895]
["TB-105S",null,"1/220/60",0.28,60,330,40,3170,58,2.4]
[null,null,"1/220/50",0.26,52,287,30,2765]
["TB-118S",null,"1/220/60",0.79,160,540,46,3150,60,6.6]
[null,null,"1/220/50",0.73,139,470,30,2760]
[null,null,"Kích thước cánh quạt (mm): TB-105S: Ø105 x 60; TB-118S: Ø118 x 60"]
["TB-105S-1",null,"1/220/60",0.28,60,330,40,3170,58,2.3]
[null,null,"1/220/50",0.26,52,287,30,2765]
["TB-118S-1",null,"1/220/60",0.79,160,540,46,3150,60,6.5]
[null,null,"1/220/50",0.73,139,470,30,2760]
[null,null,"Kích thước cánh quạt (mm): TB-105S-1: Ø105 x 60; TB-118S-1: Ø118 x 60"]
["TB-12B",null,"1/220/60",0.36,60,72,30,3440,45,2.3]
[null,null,"1/220/50",0.27,60,72,30,2890]
["TB-8B",null,"1/220/60",0.72,131,198,66,3440,60,3.5]
[null,null,"1/220/50",0.51,131,198,66,2830]
[null,null,"Kích thước cánh quạt (mm): TB-12B: Ø148 x 28; TB-8B: Ø148 x 21"]
[" TB-6B",null,"1/220/60",0.8,160,250,72,3365,62,4.7]
[null,null,"1/220/50",0.68,125,232,66,2890]
[null,null,"Kích thước cánh quạt (mm): Ø140 x 50"]
["  TB-140DS",null,"1/220/60",0.56,125,720,17,1540,62,3]
[null,null,"1/220/50",0.43,83,675,14,1230]
[null,null,"Kích thước cánh quạt (mm): Ø140 x 50"]
["(In line duct fans)"]
["TJF-15B",null,"1/220/60",0.54,117,600,42,2950,67,3.7]
[null,null,"1/220/50",0.45,95,516,32,2640]
[null,null,"Kích thước cánh quạt (mm): Ø85 x 70"]
["TJF-20B",null,"1/220/60",0.36,57,840,20,1615,54,4.5]
[null,null,"1/220/50",0.31,55,720,15,1420]
["TJF-25B",null,"1/220/60",0.43,91,1440,30,1625,58,6.8]
[null,null,"1/220/50",0.38,73,1220,23,1420]
[" TJF-30B",null,"1/220/60",2.12,240,2520,40,1660,62,10.8]
[null,null,"1/220/50",0.87,170,2140,30,1425]
["TJF-200B",null,"1/220/60",0.36,57,840,20,1615,54,5.5]
[null,null,"1/220/50",0.31,55,720,15,1420]
["TJF-250B",null,"1/220/60",0.43,91,1440,30,1625,58,8.3]
[null,null,"1/220/50",0.38,73,1220,23,1420]
[" TJF-300B",null,"1/220/60",2.12,240,2520,40,1660,62,12]
[null,null,"1/220/50",0.87,170,2140,30,1425]

{"sheet":"Quạt Windy","index":1,"n_rows":34,"n_cols":13,"rows_kept":34,"cut":false,"hidden":false,"merged":[[5,2,5,11],[6,2,6,3],[6,4,6,11],[9,2,12,2],[9,3,24,3],[9,6,10,6],[9,9,10,9],[13,2,16,2],[13,6,14,6],[13,9,14,9],[17,2,20,2],[17,6,18,6],[17,9,18,9],[13,12,14,12],[15,6,16,6],[15,9,16,9],[15,12,16,12],[9,12,10,12],[11,6,12,6],[11,9,12,9],[11,12,12,12],[21,9,22,9],[21,12,22,12],[23,6,24,6],[23,9,24,9],[23,12,24,12],[17,12,18,12],[19,6,20,6],[19,9,20,9],[19,12,20,12],[25,2,28,2],[25,3,34,3],[29,2,32,2],[33,2,34,2],[21,2,24,2],[21,6,22,6]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[null,null,"BẢNG THÔNG TIN QUẠT WINDY FAN"]
[null,null,"Sản Phẩm",null,"Thông số kỹ thuật"]
[null,null,"Model","Hình ảnh","Power\n(∮/V/Hz)","I \n(A)","D hút\n(cm)","P vào\n(W)","T. độ\n(Rpm)","P ra\n(kW)","Q \n(m3/ph)","Áp lực\n(Pa)","m\n(Kg)"]
[null,null,"Quạt tròn lưu thông không khí (Circulating Ventilator)"]
[null,null,"DCF-400",null,"1/220/50",0.8,37,125,1460,0.3,76,215,24]
[{"$nulls":4},"1/220/60",0.79,null,160,1730,null,90,295]
[{"$nulls":4},"3/220-380/50","1.4/0.8",37,170,1465,0.3,76,215,24]
[{"$nulls":4},"3/220-380/60","1.05/0.6",175,175,1735,175,90,295]
[null,null,"DCF-500",null,"1/220/50",1.15,50,360,1420,0.4,115,205,29]
[{"$nulls":4},"1/220/60",1.35,565,565,1700,565,135,295]
[{"$nulls":4},"3/220-380/50","1.30/0.75",50,355,1430,0.4,115,205,29]
[{"$nulls":4},"3/220-380/60","1.30/0.75",435,435,1700,435,135,295]
[null,null,"DCF-600",null,"1/220/50",1.65,60,290,975,0.6,210,195,33]
[{"$nulls":4},"1/220/60",1.7,375,375,1175,375,250,275]
[{"$nulls":4},"3/220-380/50","2.6/1.5",60,295,980,0.3,210,195,33]
[{"$nulls":4},"3/220-380/60","2.05/1.2",330,330,1170,330,250,275]
[null,null,"DCF-800",null,"1/220/50",4.8,80,900,965,1.5,380,275,38]
[{"$nulls":4},"1/220/60",6.6,1450,1450,1145,1450,450,295]
[{"$nulls":4},"3/220-380/50","6.7/3.85",80,980,970,1.5,380,275,38]
[{"$nulls":4},"3/220-380/60","5.8/3.35",1350,1350,1150,1350,450,295]
[null,null,"DVR-400"]
[]
[]
[]
[null,null,"DVR-500"]
[]
[]
[]
[null,null,"DVR-600"]